##
List of currently supported ICs for full testing at IC Tester device

List of test entries in database /usr/local/share/ictester/default.tdf (v1):

Test entry | Type of entry | IC true name | IC description | Confirmed test?
3003 | link to 7432 | MC 3003 | 4 x OR gates with 2 inputs | YES
4001 | test data | CD 4001 | 4 x NOR gates with 2 inputs | YES
4002 | test data | CD 4002 | 2 x NOR gates with 4 inputs | NO
40106 | link to 7404 | CD 40106 | 5 x NOT Schmitt-trigger gates | NO
4011 | test data | CD 4011 | 4 x NAND gates with 2 inputs | YES
4012 | test data | CD 4012 | 2 x NAND gates with 4 inputs | NO
4016 | link to 4066 | CD 4016 | 4 x analog switch | NO
4030 | test data | CD 4030 | 4 x XOR gates with 2 inputs | NO
4049 | test data | CD 4049 | 6 x NOT gates | YES
4066 | test data | CD 4066 | 4 x analog switch | YES
4069 | link to 7404 | CD 4069 | 6 x NOT gates | NO
4071 | test data | CD 4071 | 4 x OR gates with 2 inputs | NO
4072 | test data | CD 4072 | 2 x OR gates with 4 inputs | NO
4081 | test data | CD 4081 | 4 x AND gates with 2 inputs | YES
4082 | test data | CD 4082 | 2 x AND gates with 4 inputs | NO
4093 | link to 4011 | CD 4093 | 4 x NAND schmitt-trigger gates with 2 inputs | NO
5400 | link to 7400 | SN 5400 | 4 x NAND gates with 2 inputs | NO
5401 | link to 7401 | SN 5401 | 4 x NAND gates with 2 inputs | NO
5402 | link to 7402 | SN 5402 | 4 x NOR gates with 2 inputs | NO
5403 | link to 7400 | SN 5403 | 4 x NAND gates with 2 inputs - open collector | NO
5404 | link to 7404 | SN 5404 | 6 x NOT gates | NO
5405 | link to 7404 | SN 5405 | 6 x NOT gates - open collector | NO
5406 | link to 7404 | SN 5406 | 6 x NOT gates - open collector 30V | NO
5408 | link to 7408 | SN 5408 | 4 x AND gates with 2 inputs | NO
5409 | link to 7408 | SN 5409 | 4 x AND gates with 2 inputs - open collector | NO
5410 | link to 7410 | SN 5410 | 3 x NAND gates with 3 inputs | NO
5411 | link to 7411 | SN 5411 | 3 x AND gates with 3 inputs | NO
5412 | link to 7410 | SN 5412 | 3 x NAND gates with 3 inputs - open collector | NO
54128 | link to 7402 | SN 54128 | 4 x NOR line driver gates with 2 inputs, 50 ohma | NO
5413 | link to 7420 | SN 5413 | 2 x NAND schmitt-trigger gates with 4 inputs | NO
54132 | link to 7400 | SN 54132 | 4 x NAND schmitt-trigger gates with 2 inputs | NO
54136 | link to 7486 | SN 54136 | 4 x XOR gates with 2 inputs - open collector | NO
5414 | link to 7404 | SN 5414 | 6 x NOT Schmitt-trigger gates | NO
54145 | link to 7442 | SN 54145 | BCD to decimal decoder/driver - open collector 80 mA (max) | NO
5415 | link to 7411 | SN 5415 | 3 x AND gates with 3 inputs - open colletor | NO
5416 | link to 7404 | SN 5416 | 6 x NOT gates - open collector 15V | NO
5420 | link to 7420 | SN 5420 | 2 x NAND gates with 4 inputs | NO
5421 | link to 7421 | SN 5421 | 2 x AND gates with 4 inputs | NO
5422 | link to 7420 | SN 5422 | 2 x NAND gates with 4 inputs - open collector | NO
54246 | link to 7446 | SN 54246 | BCD to 7 segment decoder/driver - open collector 40 mA | NO
54247 | link to 7446 | SN 54247 | BCD to 7 segment decoder/driver - open collector 40 mA | NO
54248 | link to 7446 | SN 54248 | BCD to 7 segment decoder/driver | NO
5426 | link to 7400 | SN 5426 | 4 x NAND gates with 2 inputs - open collector 15V | NO
5427 | link to 7427 | SN 5427 | 3 x NOR gates with 3 inputs | NO
5428 | link to 7402 | SN 5428 | 4 x NOR gates with 2 inputs | NO
5430 | link to 7430 | SN 5430 | 1 x NAND gates with 8 inputs | NO
5432 | link to 7432 | SN 5432 | 4 x OR gates with 2 inputs | NO
5433 | link to 7402 | SN 5433 | 4 x NOR gates with 2 inputs - open collector | NO
5437 | link to 7400 | SN 5437 | 4 x NAND gates with 2 inputs | NO
5438 | link to 7400 | SN 5438 | 4 x NAND gates with 2 inputs - open collector | NO
5439 | link to 7401 | SN 5439 | 4 x NAND gates with 2 inputs | NO
5440 | link to 7420 | SN 5440 | 2 x NAND gates with 4 inputs | NO
5442 | link to 7442 | SN 5442 | BCD to decimal decoder | NO
5443 | link to 7443 | SN 5443 | Excess 3 to decimal decoder | NO
5444 | link to 7444 | SN 5444 | Excess 3-Gray to decimal decoder | NO
5445 | link to 7445 | SN 5445 | BCD to decimal decoder - open collector | NO
5446 | link to 7446 | SN 5446 | BCD to 7 segment decoder/driver - open collector 30V | NO
5447 | link to 7446 | SN 5447 | BCD to 7 segment decoder/driver - open collector 15V | NO
5448 | link to 7446 | SN 5448 | BCD to 7 segment decoder/driver | NO
5486 | link to 7486 | SN 5486 | 4 x XOR gates with 2 inputs | NO
54LS347 | link to 7446 | SN 54LS347 | BCD to 7 segment decoder/pointer driver - open collector 7V | NO
54LS447 | link to 7446 | SN 54LS447 | BCD to 7 segment decoder/driver - open collector 7V | NO
55451 | link to 75451 | SN 55451 | 2 x AND gates with 2 inputs | NO
55452 | link to 75452 | SN 55452 | 2 x NAND gates with 2 inputs | NO
55453 | link to 75453 | SN 55453 | 2 x OR gates with 2 inputs | NO
55454 | link to 75454 | SN 55454 | 2 x NOR gates with 2 inputs | NO
7400 | test data | SN 7400 | 4 x NAND gates with 2 inputs | YES
7401 | test data | SN 7401 | 4 x NAND gates with 2 inputs | NO
7402 | test data | SN 7402 | 4 x NOR gates with 2 inputs | YES
7403 | link to 7400 | SN 7403 | 4 x NAND gates with 2 inputs - open collector | YES
7404 | test data | SN 7404 | 6 x NOT gates | YES
7405 | link to 7404 | SN 7405 | 6 x NOT gates - open collector | NO
7406 | link to 7404 | SN 7406 | 6 x NOT gates/driver - open collector 30V | NO
7408 | test data | SN 7408 | 4 x AND gates with 2 inputs | YES
7409 | link to 7408 | SN 7409 | 4 x AND gates with 2 inputs - open collector | NO
7410 | test data | SN 7410 | 3 x NAND gates with 3 inputs | YES
7411 | test data | SN 7411 | 3 x AND gates with 3 inputs | NO
7412 | link to 7410 | SN 7412 | 3 x NAND gates with 3 inputs - open collector | YES
74128 | link to 7402 | SN 74128 | 4 x NOR gates with 2 inputs - line driver 50 ohm | NO
7413 | link to 7420 | SN 7413 | 2 x NAND schmitt trigger gates with 4 inputs | NO
74132 | link to 7400 | SN 74132 | 4 x NAND schmitt trigger gates with 2 inputs | YES
74136 | link to 7486 | SN 74136 | 4 x XOR gates with 2 inputs - open collector | NO
7414 | link to 7404 | SN 7414 | 6 x NOT schmitt trigger gates | NO
74145 | link to 7442 | SN 74145 | BCD to decimal decoder/driver - open collector 80 mA (max) | NO
7416 | link to 7404 | SN 7416 | 6 x NOT gates - open collector 15V | YES
7420 | test data | SN 7420 | 2 x NAND gates with 4 inputs | YES
7421 | test data | SN 7421 | 2 x AND gates with 4 inputs | NO
7422 | link to 7420 | SN 7422 | 2 x NAND gates with 4 inputs - open collector | NO
74246 | link to 7446 | SN 74246 | BCD to 7 segment decoder/driver - open collector 80 mA | NO
74247 | link to 7446 | SN 74247 | BCD to 7 segment decoder/driver - open collector 40 mA | NO
74248 | link to 7446 | SN 74248 | BCD to 7 segment decoder/driver | NO
7426 | link to 7400 | SN 7426 | 4 x NAND gates with 2 inputs - open collector 15V | NO
7427 | test data | SN 7427 | 3 x NOR gates with 3 inputs | NO
7428 | link to 7402 | SN 7428 | 4 x NOR gates with 2 inputs | NO
7430 | test data | SN 7430 | 1 x NAND gates with 8 inputs | YES
7432 | test data | SN 7432 | 4 x OR gates with 2 inputs | NO
7433 | link to 7402 | SN 7433 | 4 x NOR gates with 2 inputs - open collector | NO
7437 | link to 7400 | SN 7437 | 4 x NAND gates with 2 inputs/driver | YES
7438 | link to 7400 | SN 7438 | 4 x NAND gates with 2 inputs/driver - open collector | YES
7439 | link to 7401 | SN 7439 | 4 x NAND gates with 2 inputs/driver | NO
7440 | link to 7420 | SN 7440 | 2 x NAND gates with 4 inputs/driver | YES
7442 | test data | SN 7442 | BCD to decimal decoder | YES
7443 | test data | SN 7443 | Excess-3 to decimal decoder | NO
7444 | test data | SN 7444 | Excess-3 gray to decimal decoder | NO
7445 | link to 7442 | SN 7445 | BCD to decimal decoder/driver - open collector 30V | NO
7446 | test data | SN 7446 | BCD to 7 segment decoder/driver | NO
7447 | link to 7446 | SN 7447 | BCD to 7 segment decoder/driver - open collector 15V | YES
7448 | link to 7446 | SN 7448 | BCD to 7 segment decoder/driver | NO
7486 | test data | SN 7486 | 4 x XOR gates with 2 inputs | YES
74LS00 | link to 7400 | SN 74LS00 | 4 x NAND gates with 2 inputs | YES
74LS02 | link to 7402 | SN 74LS02 | 4 x NOR gates with 2 inputs | YES
74LS04 | link to 7404 | SN 74LS04 | 6 x NOT gates | YES
74LS08 | link to 7408 | SN 74LS09 | 4 x AND gates with 2 inputs | YES
74LS132 | link to 7400 | SN 74LS132 | 4 x NAND schmitt trigger gates with 2 inputs | YES
74LS15 | link to 7411 | SN 74LS15 | 3 x AND gates with 3 inputs - open collector | NO
74LS30 | link to 7430 | SN 74LS30 | 1 x NAND gates with 8 inputs | YES
74LS32 | link to 7432 | SN 74LS32 | 4 x OR gates with 2 inputs | YES
74LS347 | link to 7446 | SN 74LS347 | BCD to 7 segment decoder/pointer driver - open collector 7V | NO
74LS447 | link to 7446 | SN 74LS447 | BCD to 7 segment decoder/pointer driver - open collector 7V | NO
74LS86 | link to 7486 | SN 74LS86 | 4 x XOR gates with 2 inputs | YES
75140 | test data | SN 75140 | 2 x Line receiver | YES
75451 | test data | SN 75451 | 2 x AND gates with 2 inputs | NO
75452 | test data | SN 75452 | 2 x NAND gates with 2 inputs | NO
75453 | test data | SN 75453 | 2 x OR gates with 2 inputs | YES
75454 | test data | SN 75454 | 2 x NOR gates with 2 inputs | NO